AIGUI Variablen und Properties

|  |  |  |  |
| --- | --- | --- | --- |
| State | Property | Default | Description |
| Initialization | workingDirectory | The current Dir. |  |
|  | optionsDataN | optionsDataN | Initialization commands |
| ReadNetlist | Netlist | netlistN | The loaded netlist |
| CircuitEquations | variablesData | - | Number of variables |
|  | variablesDataN | - | N-th variable |
|  | analyzedSignal | - |  |
|  | MatrixEquations | equationsN | The circuit matrix equations |
| ApproximateTransferFunction | Function | approximateTransferFunctionN |  |
| NDAESolve | NDAESolution | transienteN |  |
| Solve | Function | solvedFunctionN |  |

## Initialization

{optionsDataN}

SetOptions[ AnalogInsydes {,options}]

## ReadNetlist